***Price + Service + Support = Value***

**Up to 50 Rooms $7995 Includes**  
4 admin IP phones  
up to 72 Analog Ports  
36 month Auto Renew **MRC $300**   
All Domestic calling with 2 inbound numbers   
Maintenance on the PBX and Related Equipment

**51 to 100 Rooms $9995** **Includes** 5 admin IP phones  
Up to 120 Analog Ports  
36 month Auto Renew **MRC $400**  
All Domestic calling with 5 inbound numbers   
Maintenance on PBX and Related Equipment

**101 to 150 rooms $12995**   
6 admin IP phones  
Up to 168 Analog Ports  
36 month Auto Renew MRC $475  
All Domestic calling with 5 inbound numbers   
Maintenance on PBX and Related Equipment

**151 to 200 rooms $15,995**10 admin IP phones  
Up to 216 Analog Ports  
36 month Auto Renew **MRC $525**   
All Domestic calling with 6 inbound numbers   
Maintenance on PBX and Related Equipment

**201 to 250 rooms $19,995**   
10 admin IP phones  
Up to 264 Analog Ports  
36 month Auto Renew MRC $625  
All Domestic calling with 10 inbound numbers   
Maintenance on PBX and Related Equipment

**251 to 300 rooms $23,995**   
12 admin IP phones  
up to 312 Analog Ports  
36 month Auto Renew MRC $700   
All domestic calling with 10 inbound numbers   
Maintenance on PBX and Related Equipment

*Please contact us for quotes for properties over 300 rooms or SIP Installations*

*All offers include a mix of admin IP phones either Sangoma 4xx and 5xx or Yeastar T42s and T46s models. All PBX Systems are built assuming the use of analog phones in Guest Rooms. PMS interface is built to Hitachi or Mitel standards. All MRC monies to be paid via a pre-authorized (ACH or Credit Card) payment system, invoiced monthly on 1st of the month. Prices shown do not include taxes. Travel outside of NYC Tristate area will be additional charge. Building cabling will not be covered by agreement unless installed by Jetcom or its affiliates. All the above offers are non-binding to both Jetcom and potential client. Jetcom reserves the right to at any time remove these offers for any reason with no notice required.*